#
DIFFERENTIAL DISASSEMBLY

D6E051527100102

1. Disassemble in the order shown in the figure.

1 | Bearing (ring gear side) (See Bearing (Ring Gear Side) Disassembly Note.)
2 | Bearing (ring gear-opposite side) (See Bearing (Ring Gear-Opposite Side) Disassembly Note (4X2).) (See Bearing (Ring Gear-Opposite Side) Disassembly Note (4X4).)
3 | Ring gear
4 | Gear case component

## Bearing (Ring Gear Side) Disassembly Note

1. Remove the bearing using the SST.

## Bearing (Ring Gear-Opposite Side) Disassembly Note (4X2)

1. Remove the bearing using the SST.

## Bearing (Ring Gear-Opposite Side) Disassembly Note (4X4)

1. Remove the bearing roller guide by prying with a flathead screwdriver as shown in the figure.

2. Remove the bearing inner race using the SSTs.