#
CRUISE CONTROL SWITCH INSPECTION [L8, LF, L3, L3 Turbo]

id0120a5800100

1. Disconnect the negative battery cable.

2. Remove the driver-side air bag module. (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

3. Disconnect the cruise control switch connector.

4. Inspect for resistance and continuity between the cruise control switch terminals using an ohmmeter.

  • If not as specified, replace the cruise control switch.