HEADLIGHT AIMING

id091800464000

Low-beam

1. Point the headlight beams to a wall and verify that the headlight beams are as shown in the figure.

am6zzw00003798

2. Make a headlight adjustment screen as shown in the figure using double-weight, white paper.

am6zzw00008684

3. Adjust the tire pressure to the specification.

4. Position the unloaded vehicle on a flat, level surface.

5. Sit on the driver-side seat alone.

6. Line up the headlights with the wall at a distance of 3 m {9.8 ft} apart.

am6zzw00008632

7. Measure the height of A (the lower end of the line) shown in the figure from the surface which the tires are set.

am6zzw00008653

  Note
  • The height of the headlight center point is the value actually measured plus 50 mm {2.0 in} because the headlight center point is not embossed on the cover.

8. Align the center of the headlight with the center of the screen.

am6zzw00008663

9. Block the light of the headlight which is not adjusted.

10. Start the engine and charge the battery.

11. Turn on the headlight low beams.

12. Set the headlight leveling switch to the 0 position. (vehicles with headlight leveling switch)

13. Verify that the elbow point of the headlight is in the position indicated on the screen.

  • If the elbow point is not at the position indicated by the adjustment screen, turn the adjustment screw as shown in the figure to adjust the elbow point to the position indicated by the adjustment screen.

  am6zzw00008635

am6zzw00008636

am6zzw00008637

High-beam

1. Adjust the tire air pressure to the specification.

2. Position the unloaded vehicle on a flat, level surface.

3. Seat one person in the driver"s seat.

4. Position the vehicle straight ahead and perpendicular to a wall.

5. Set the headlights 3 m {10 ft} from the wall.

am6zzw00008638

6. Measure the height of A (the lower end of the line) shown in the figure from the surface which the tires are set.

am6zzw00008653

  Note
  • The height of the headlight center point is the value actually measured plus 50 mm {2.0 in} because the headlight center point is not embossed on the cover.

7. Align the center of the headlight with the center of the screen.

am6zzw00008664

8. Start the engine to charge the battery.

9. Turn on the high-beam headlights.

10. Set the headlight leveling switch to 0 position.

11. Adjust the headlights as shown in the figure.

am6zzw00008640

am6zzw00008639