#
FRONT FOG LIGHT REMOVAL/INSTALLATION

id091800468500

  Note

  • Front fog light (TYPE A) is built in the front combination light.

## Type B

1. Disconnect the negative battery cable.

2. Remove the under cover.

3. Slightly bend back the mudguard.

4. Remove in the order indicated in the table.

1 | Connector
2 | Screw
3 | Front fog light

5. Install in the reverse order of removal.

6. Adjust the front fog light aiming. (See FRONT FOG LIGHT AIMING.)