#
DTC C1507, C1508 [DSC]

id040220875100

DTC | C1507 C1508 | DSC control
DETECTION CONDITION | • C1507: - Brake TCS or DSC controls continue operation for 20 s or more • C1508: - Engine TCS control continues operation for 60 s or more
POSSIBLE CAUSE | • System is normal For protection of solenoid valves in the DSC HU/CM, or protection of the engine, sustained and continual control of DSC and TCS is inhibited

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY CURRENT STATUS OF MALFUNCTION • Clear DTC from memory. (See Clearing DTCs Procedures) • Start engine and drive vehicle at 10 km/h {6.2 mph} or above. • Is same DTC present? | Yes | Replace DSC HU/CM, then go to next step.
No | Inspect intermittent concern using the same procedure as engine control system.
2 | VERIFY THAT NO OTHER DTCS ARE PRESENT • Are any other DTCs output? | Yes | Go to the applicable DTC inspection. (See DTC Table.)
No | DTC troubleshooting completed.