OIL JET VALVE INSPECTION

id011000505900

MZR 2.0 DISI, MZR 2.0 DISI i-stop

1. Apply compressed air to oil jet valve A and verify that air passes through oil jet valve B.

  • If air does not flow, replace the oil jet valve.

belbze00000104

  Air pressure

  0.22—0.27 MPa {2.3—2.7 kgf/cm2 32—39 psi}

MZR 2.3 DISI Turbo

1. Apply compressed air to oil jet valve A and verify that air passes through oil jet valve B.

  • If air does not flow, replace the oil jet valve.

beltze00000022

  Air pressure

  0.17—0.23 MPa {1.8—2.3 kgf/cm2 25—33 psi}