#
FRONT DOOR UNIT REMOVAL/INSTALLATION

id091100800500

1. Remove the front door glass. (See FRONT DOOR GLASS REMOVAL/INSTALLATION.)

2. Remove the inner handle. (See INNER HANDLE REMOVAL/INSTALLATION.)

3. Remove the front door speaker. (See FRONT DOOR SPEAKER REMOVAL/INSTALLATION.)

4. Disconnect the power window motor connector, front door lock actuator connector, power outside mirror connector.

5. Remove the door harness from the front door unit.

6. Remove the bolts.

7. Remove the screw.

8. Remove the front door actuator hook from the front door module.

9. Pull the front door unit slightly towards you, and while keeping the power window regulator from catching on the door, remove the door unit from the door.

10. Pull out the inner handle cable and door lock knob cable from the hole.

11. Remove the power window motor and power window regulator from the door module.

12. Install in the reverse order of removal.