#
ENGINE OIL LEVEL INSPECTION [MZR-CD (RF Turbo)]

id0111f1800500

  Note

  • The amount of engine oil may increase if fuel is mixed into the engine oil while removing particulate matter accumulated in the diesel particulate filter, however, it does not indicate an abnormality.

1. Position the vehicle on level ground.

2. Warm up the engine to normal operating temperature.

3. Stop the engine and wait for 10 min.

4. Verify that the oil level is between the X and L marks on the dipstick and check the engine oil condition.

  • If the oil level is below the L mark, add engine oil. (See ENGINE OIL REPLACEMENT [MZR-CD (RF Turbo)].)
  • If the oil level is close to or exceeds the X mark, replace the engine oil. (See ENGINE OIL REPLACEMENT [MZR-CD (RF Turbo)].)