#
GENERATOR REMOVAL/INSTALLATION [L3 Turbo]

id0117b18002b2

  Warning

  • When the battery cables are connected, touching the vehicle body with generator terminal B will generate sparks. This can cause personal injury, fire, and damage to the electrical components. Always disconnect the battery negative cable before performing the following operation.

  Caution

  • The generator can be damaged by the heat from the exhaust manifold. Make sure the generator duct is installed securely.

## L.H.D.

1. Disconnect the negative battery cable.

2. Remove the under cover.

3. Remove the drive belt. (See DRIVE BELT REPLACEMENT [L3 Turbo].)

4. Remove the charge air cooler cover. (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L3 Turbo].)

5. Remove the cowl panel. (See COWL PANEL REMOVAL/INSTALLATION.)

6. Remove in the order indicated in the table.

7. Install in the reverse order of removal.

.

1 | Generator duct
2 | Terminal B cable
3 | Generator connector
4 | Generator (See Generator Removal Note (L.H.D.).) (See Generator Installation Note (L.H.D.).)

## Generator Removal Note (L.H.D.)

1. Remove the generator from above the engine compartment.

## Generator Installation Note (L.H.D.)

1. Tighten bolt A temporarily.

2. Tighten bolt B, C to the specified tightening torque.

3. Tighten bolt A to the specified tightening torque.

## R.H.D.

1. Disconnect the negative battery cable.

2. Remove the under cover.

3. Remove the drive belt. (See DRIVE BELT REPLACEMENT [L3 Turbo].)

4. Remove the charge air cooler. (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L3 Turbo].)

5. Remove the heat insulator (master cylinder side). (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L3 Turbo].)

6. Disconnect the front drive shaft (RH) from the joint shaft. (See FRONT DRIVE SHAFT REMOVAL/INSTALLATION [L3 Turbo].)

7. Remove in the order indicated in the table.

8. Install in the reverse order of removal.

.

1 | Exhaust manifold bracket
2 | Generator duct
3 | Terminal B cable
4 | Generator connector
5 | Generator (See Generator Removal Note (R.H.D.).) (See Generator Installation Note (R.H.D.).)

## Generator Removal Note (R.H.D.)

1. Remove the generator from below the engine compartment.

## Generator Installation Note (R.H.D.)

1. Tighten bolt A temporarily.

2. Tighten bolt B, C to the specified tightening torque.

3. Tighten bolt A to the specified tightening torque.