#
GLASS PANEL ADJUSTMENT

id091500800600

1. Fully close the glass panel.

2. Measure the gap and height between the glass panel and body.

3. If not as specified, loosen the glass panel installation screws and reposition the glass panel.

Clearance

  a: -0.8-1.2 mm {-0.031-0.047 in}
  b: -0.8-1.2 mm {-0.031-0.047 in}
  c: 1.0-3.0 mm {0.04-0.11 in}
  d: 1.1-3.1 mm {0.044-0.12 in}
  e: 0 mm {0 in}

4. Tighten the installation screws.

5. Insert any available thin plastic card between the weatherstrip and the body, and verify that they are sealed. (There is resistance when the plastic card is moved.)

  • If they are not sealed, perform Steps 3-4 and adjust again.