#
SHIFT INTERLOCK MECHANISM OPERATION [G66M-R]

id0515k1101400

## Structure

• During shifting, the shift rods, except for the one in operation, are locked in the neutral position by the interlock sleeve.

### Neutral condition

  • The interlock sleeve fits into the notches of the 1st/2nd, 5th/6th and reverse shift forks.
  The control lever fits into the notch of the 3rd/4th shift fork.

.

1 | Shift fork
2 | Interlock sleeve
3 | Control lever
4 | Shift fork

### Select condition

  • The shift lever is moved laterally to the 1st/2nd position.
  Both the control lever and the interlock sleeve turn in the direct shown by the arrow.
  The control lever fits into the notch of the 1st/2nd shift fork.
  The interlock sleeve fits into the notches of the 3rd/4th, 5th/6th and reverse shift forks.

.

1 | Shift fork (1st/2nd)

### Shift condition

  • The shift lever is moved vertically to the 2nd position.
  The control lever moves up the 1st/2nd shift fork and the change to 2nd gear is complete.
  The interlock sleeve holds the 3rd/4th, 5th/6th and reverse shift forks at the neutral position, preventing double engagement of gears.
  The operation procedure is the same for other gear positions.

.

1 | Shift fork (5th/6th)
2 | Shift fork (3rd/4th)
3 | Shift fork (reverse)