#
DTC TABLE [L3 Turbo]

id0102b7545200
×: Applicable
-: Not applicable

DTC No. | Condition | MIL | DC | Monitor item | Self-test type*2 | Memory function | Page
--- | --- | --- | --- | --- | --- | --- | ---
P0011 | CMP Timing over-advanced | ON | 1 | CCM | C, R | × | (See DTC P0011 [L3 Turbo].)
P0012 | CMP Timing over-retarded | ON | 2 | CCM | C, R | × | (See DTC P0012 [L3 Turbo].)
P0030 | A/F sensor heater control circuit problem | ON | 2 | A/F sensor heater, HO2S heater | C, O, R | × | (See DTC P0030 [L3 Turbo].)
P0031 | A/F sensor heater circuit low input | ON | 2 | A/F sensor heater, HO2S heater | C, O, R | × | (See DTC P0031 [L3 Turbo].)
P0032 | A/F sensor heater circuit high input | ON | 2 | A/F sensor heater, HO2S heater | C, O, R | × | (See DTC P0032 [L3 Turbo].)
P0037 | HO2S heater circuit low input | ON | 2 | A/F sensor heater, HO2S heater | C, O, R | × | (See DTC P0037 [L3 Turbo].)
P0038 | HO2S heater circuit high input | ON | 2 | A/F sensor heater, HO2S heater | C, O, R | × | (See DTC P0038 [L3 Turbo].)
P0069 | Manifold absolute pressure/atmospheric pressure correlation | ON | 2 | CCM | C | × | (See DTC P0069 [L3 Turbo].)
P0089 | Fuel pressure regulator performance | OFF | 1 | Other | C, O, R | × | (See DTC P0089 [L3 Turbo].)
P0091 | Fuel pressure regulator control circuit low | ON | 1 | CCM | C, O, R | × | (See DTC P0091 [L3 Turbo].)
P0092 | Fuel pressure regulator control circuit high | ON | 1 | CCM | C, O, R | × | (See DTC P0092 [L3 Turbo].)
P0096 | IAT sensor 2 circuit range/performance problem | ON | 2 | CCM | C | × | (See DTC P0096 [L3 Turbo].)
P0097 | IAT sensor 2 circuit low | ON | 1 | CCM | C, O, R | × | (See DTC P0097 [L3 Turbo].)
P0098 | IAT sensor 2 circuit high | ON | 1 | CCM | C, O, R | × | (See DTC P0098 [L3 Turbo].)
P0101 | MAF circuit range/performance problem | ON | 2 | CCM | C | × | (See DTC P0101 [L3 Turbo].)
P0102 | MAF circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P0102 [L3 Turbo].)
P0103 | MAF circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P0103 [L3 Turbo].)
P0107 | MAP sensor circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P0107 [L3 Turbo].)
P0108 | MAP sensor circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P0108 [L3 Turbo].)
P0111 | IAT circuit performance problem | ON | 2 | CCM | C | × | (See DTC P0111 [L3 Turbo].)
P0112 | IAT circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P0112 [L3 Turbo].)
P0113 | IAT circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P0113 [L3 Turbo].)
P0117 | ECT circuit low input | ON | 1 | Engine cooling system | C, O, R | × | (See DTC P0117 [L3 Turbo].)
P0118 | ECT circuit high input | ON | 1 | Engine cooling system | C, O, R | × | (See DTC P0118 [L3 Turbo].)
P0122 | TP sensor No.1 circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P0122 [L3 Turbo].)
P0123 | TP sensor No.1 circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P0123 [L3 Turbo].)
P0125 | Excessive time to enter closed loop fuel control | ON | 2 | Engine cooling system | C | × | (See DTC P0125 [L3 Turbo].)
P0131 | A/F sensor circuit low input | ON | 2 | A/F sensor, HO2S | C, O, R | × | (See DTC P0131 [L3 Turbo].)
P0132 | A/F sensor circuit high input | ON | 2 | A/F sensor, HO2S | C, O, R | × | (See DTC P0132 [L3 Turbo].)
P0133 | A/F sensor circuit problem | ON | 2 | A/F sensor, HO2S | C | × | (See DTC P0133 [L3 Turbo].)
P0134 | A/F sensor circuit no activity detected | ON | 2 | A/F sensor, HO2S | C, R | × | (See DTC P0134 [L3 Turbo].)
P0138 | HO2S circuit high input | ON | 2 | A/F sensor, HO2S | C, O, R | × | (See DTC P0138 [L3 Turbo].)
P0140 | HO2S circuit no activity detected | ON | 2 | A/F sensor, HO2S | C, R | × | (See DTC P0140 [L3 Turbo].)
P0192 | Fuel rail pressure sensor circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P0192 [L3 Turbo].)
P0193 | Fuel rail pressure sensor circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P0193 [L3 Turbo].)
P0201 | Injector circuit/open cylinder No.1 | ON | 1 | CCM | C, R | × | (See DTC P0201 [L3 Turbo].)
P0202 | Injector circuit/open cylinder No.2 | ON | 1 | CCM | C, R | × | (See DTC P0202 [L3 Turbo].)
P0203 | Injector circuit/open cylinder No.3 | ON | 1 | CCM | C, R | × | (See DTC P0203 [L3 Turbo].)
P0204 | Injector circuit/open cylinder No.4 | ON | 1 | CCM | C, R | × | (See DTC P0204 [L3 Turbo].)
P0222 | TP sensor No.2 circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P0222 [L3 Turbo].)
P0223 | TP sensor No.2 circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P0223 [L3 Turbo].)
P0234 | Turbo/supercharger overboost condition | OFF | 1 | Other | C, R | × | (See DTC P0234 [L3 Turbo].)
P0245 | Turbocharger wastegate solenoid low | OFF | 2 | Other | C, O, R | × | (See DTC P0245 [L3 Turbo].)
P0246 | Turbocharger wastegate solenoid high | OFF | 2 | Other | C, O, R | × | (See DTC P0246 [L3 Turbo].)
P0300 | Random misfire detected | Flash / ON | 1 or 2 | Misfire | C, R | × | (See DTC P0300 [L3 Turbo].)
P0301 | Cylinder No.1 misfire detected | Flash / ON | 1 or 2 | Misfire | C, R | × | (See DTC P0301, P0302, P0303, P0304 [L3 Turbo].)
P0302 | Cylinder No.2 misfire detected | Flash / ON | 1 or 2 | Misfire | C, R | × | (See DTC P0301, P0302, P0303, P0304 [L3 Turbo].)
P0303 | Cylinder No.3 misfire detected | Flash / ON | 1 or 2 | Misfire | C, R | × | (See DTC P0301, P0302, P0303, P0304 [L3 Turbo].)
P0304 | Cylinder No.4 misfire detected | Flash / ON | 1 or 2 | Misfire | C, R | × | (See DTC P0301, P0302, P0303, P0304 [L3 Turbo].)
P0327 | Knock sensor circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P0327 [L3 Turbo].)
P0328 | Knock sensor circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P0328 [L3 Turbo].)
P0335 | CKP sensor circuit malfunction | ON | 1 | CCM | C | × | (See DTC P0335 [L3 Turbo].)
P0340 | CMP sensor circuit malfunction | ON | 1 | CCM | C | × | (See DTC P0340 [L3 Turbo].)
P0403 | EGR valve (stepper motor) circuit malfunction | ON | 2 | CCM | C, O, R | × | (See DTC P0403 [L3 Turbo].)
P0421 | Catalyst system efficiency below threshold | ON | 2 | Catalyst | C | × | (See DTC P0421 [L3 Turbo].)
P0443 | EVAP control system purge control valve circuit malfunction | ON | 2 | CCM | C, O, R | × | (See DTC P0443 [L3 Turbo].)
P0480 | Fan relay No.1 control circuit malfunction | OFF | 1 | Other | C, O, R | × | (See DTC P0480 [L3 Turbo].)
P0500 | Vehicle speed sensor (VSS) circuit malfunction | ON | 2 | CCM | C | × | (See DTC P0500 [L3 Turbo].)
P0505 | Idle control system malfunction | OFF | - | - | R | - | (See DTC P0505 [L3 Turbo].)
P0506 | Idle control system RPM lower than expected | ON | 2 | CCM | C | × | (See DTC P0506 [L3 Turbo].)
P0507 | Idle control system RPM higher than expected | ON | 2 | CCM | C | × | (See DTC P0507 [L3 Turbo].)
P0550 | PSP switch circuit malfunction | ON | 2 | CCM | C | × | (See DTC P0550 [L3 Turbo].)
P0564 | Cruise control switch circuit malfunction | OFF | 1 | Other | C | × | (See DTC P0564 [L3 Turbo].)
P0571 | Brake switch circuit malfunction | OFF | 1 | Other | C | × | (See DTC P0571 [L3 Turbo].)
P0601 | Internal control module memory check sum error | ON | 1 | CCM | C, O, R | × | (See DTC P0601 [L3 Turbo].)
P0602 | PCM programming error | ON | 1 | CCM | C, O, R | × | (See DTC P0602 [L3 Turbo].)
P0604 | PCM RAM error | ON | 1 | CCM | C, O, R | × | (See DTC P0604 [L3 Turbo].)
P0606 | PCM processor | ON | 1 | CCM | C, O, R | × | (See DTC P0606 [L3 Turbo].)
P0607 | Control module performance | OFF | 1 | Other | C, O, R | × | (See DTC P0607 [L3 Turbo].)
P0610 | Control module vehicle options error | ON | 1 | CCM | C, O, R | × | (See DTC P0610 [L3 Turbo].)
P0611 | Fuel injector control module performance | OFF | 1 | Other | C, O, R | × | (See DTC P0611 [L3 Turbo].)
P0638 | Throttle actuator control range/performance | ON | 1 | CCM | C | × | (See DTC P0638 [L3 Turbo].)
P0703 | Brake switch No.1 circuit malfunction | ON | 2 | CCM | C | × | (See DTC P0703 [L3 Turbo].)
P0704 | Clutch switch circuit malfunction | ON | 2 | CCM | C | × | (See DTC P0704 [L3 Turbo].)
P0850 | Neutral switch circuit malfunction | ON | 2 | CCM | C | × | (See DTC P0850 [L3 Turbo].)
P2006 | Variable swirl control system shutter valve stuck closed | ON | 2 | CCM | C, R | × | (See DTC P2006 [L3 Turbo].)
P2009 | Variable swirl solenoid valve control circuit low | ON | 2 | CCM | C, O, R | × | (See DTC P2009 [L3 Turbo].)
P2010 | Variable swirl solenoid valve control circuit high | ON | 2 | CCM | C, O, R | × | (See DTC P2010 [L3 Turbo].)
P2088 | OCV actuator circuit low | ON | 1 | CCM | C, O, R | × | (See DTC P2088 [L3 Turbo].)
P2089 | OCV actuator circuit high | ON | 1 | CCM | C, O, R | × | (See DTC P2089 [L3 Turbo].)
P2096 | Target A/F feedback system too lean | ON | 2 | Fuel system | C | × | (See DTC P2096 [L3 Turbo].)
P2097 | Target A/F feedback system too rich | ON | 2 | Fuel system | C | × | (See DTC P2097 [L3 Turbo].)
P2100 | Throttle actuator circuit open | ON | 1 | CCM | C, O, R | × | (See DTC P2100 [L3 Turbo].)
P2101 | Throttle actuator circuit range/performance | ON | 1 | CCM | C, R | × | (See DTC P2101 [L3 Turbo].)
P2102 | Throttle actuator circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P2102 [L3 Turbo].)
P2103 | Throttle actuator circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P2103 [L3 Turbo].)
P2107 | Throttle actuator control module processor problem | ON | 1 | CCM | C, R | × | (See DTC P2107 [L3 Turbo].)
P2108 | Throttle actuator control module performance problem | ON | 1 | CCM | C, R | × | (See DTC P2108 [L3 Turbo].)
P2119 | Throttle actuator control throttle body range/performance | ON | 1 | CCM | C, R | × | (See DTC P2119 [L3 Turbo].)
P2122 | Accelerator pedal position (APP) sensor No.1 circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P2122 [L3 Turbo].)
P2123 | Accelerator pedal position (APP) sensor No.1 circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P2123 [L3 Turbo].)
P2127 | Accelerator pedal position (APP) sensor No.2 circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P2127 [L3 Turbo].)
P2128 | Accelerator pedal position (APP) sensor No.2 circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P2128 [L3 Turbo].)
P2135 | Throttle position sensor No.1/No.2 voltage correlation problem | ON | 1 | CCM | C, O, R | × | (See DTC P2135 [L3 Turbo].)
P2138 | Accelerator pedal position (APP) sensor No.1/No.2 voltage correlation problem | ON | 1 | CCM | C, O, R | × | (See DTC P2138 [L3 Turbo].)
P2177 | Fuel system too lean at off idle | ON | 2 | Fuel system | C, R | × | (See DTC P2177 [L3 Turbo].)
P2178 | Fuel system too rich at off idle | ON | 2 | Fuel system | C, R | × | (See DTC P2178 [L3 Turbo].)
P2187 | Fuel system too lean at idle | ON | 2 | Fuel system | C, R | × | (See DTC P2187 [L3 Turbo].)
P2188 | Fuel system too rich at idle | ON | 2 | Fuel system | C, R | × | (See DTC P2188 [L3 Turbo].)
P2195 | A/F sensor signal stuck lean | ON | 2 | A/F sensor, HO2S | C | × | (See DTC P2195 [L3 Turbo].)
P2196 | A/F sensor signal stuck rich | ON | 2 | A/F sensor, HO2S | C | × | (See DTC P2196 [L3 Turbo].)
P2228 | BARO sensor circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P2228 [L3 Turbo].)
P2229 | BARO sensor circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P2229 [L3 Turbo].)
P2237 | A/F sensor positive current control circuit open | ON | 2 | A/F sensor, HO2S | C, O, R | × | (See DTC P2237 [L3 Turbo].)
P2245 | A/F sensor reference voltage circuit low input | ON | 2 | A/F sensor, HO2S | C, O, R | × | (See DTC P2245 [L3 Turbo].)
P2246 | A/F sensor reference voltage circuit high input | ON | 2 | A/F sensor, HO2S | C, O, R | × | (See DTC P2246 [L3 Turbo].)
P2251 | A/F sensor negative current control circuit open | ON | 2 | A/F sensor, HO2S | C, O, R | × | (See DTC P2251 [L3 Turbo].)
P2502 | Generator terminal B circuit open | OFF | 1 | - | C, R | × | (See DTC P2502 [L3 Turbo].)
P2503 | Generator output voltage signal no electricity | OFF | 1 | Other | C, R | × | (See DTC P2503 [L3 Turbo].)
P2504 | Battery overcharge | OFF | 1 | Other | C, R | × | (See DTC P2504 [L3 Turbo].)
P2507 | PCM +BB (back-up battery) voltage low | ON | 1 | CCM | C, O, R | × | (See DTC P2507 [L3 Turbo].)
U0073 | CAN system communication error | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM].)
U0121 | Communication error to ABS HU/CM | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM].)
U0155 | Communication error to instrument cluster | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM].)

  *1 :
California emission regulation applicable model
  *2 :
C; CMDTC self-test, O; KOEO self-test, R; KOER self-test