#
AUDIO SYSTEM OUTLINE

id092000111000

• The center panel module installed with the audio unit and climate control unit (automatic A/C only), and the audio switch, A/C switch, hazard warning switch and rear window defroster switch built into the center panel has been adopted.

• A music HDD (hard disc drive) type audio unit has been adopted.

• The audio unit consists of the following parts:

  - Base unit
  Type A (BOSE)

  - AM/FM tuner
  - CD player
  - HDD (hard disc drive)
  - RDS

  Type B (BOSE)

  - AM/FM tuner
  - CD player
  - RDS

  Type C (BOSE)

  - AM/FM tuner
  - CD player

  Type D

  - AM/FM tuner
  - CD player
  - RDS

  Type E

  - AM/FM tuner
  - CD player

  - Lower module (cassette deck or MD player) (without Type A (music HDD) models)
  - Cover

• Lower module (cassette deck or MD player) are options. (without HDD)

• Module availability depends on vehicle grade.

• The following speakers have been adopted for standard specification vehicles (6 speakers):

  - Front door speaker
  - Rear door speaker
  - Tweeter*

• The following speakers have been adopted for BOSE specification vehicles (7 speakers):

  - Front door speaker
  - Rear door speaker
  - Tweeter
  - Woofer

• The audio control switch is equipped on the steering wheel for audio operation.

• A noise filter has been installed on the brake light and rear window defroster circuit, and a condenser has been installed on the high-mount brake light and rear wiper motor circuit for improved noise reduction.

• All information related to the audio system appears on the information display's LCD.

  * :
May or may not be equipped, depending on the vehicle.

## Specifications

### Audio unit

Item | Specification
--- | ---
BOSE | Standard
Type A | Type B | Type C | Type D | Type E
Rated voltage | (V) | 12
Frequency band | AM | LW | (kHz) | 153-279 | - | 153-279 | -
MW | (kHz) | 531-1602 | 522-1629 | 531-1602 | 522-1629/ 530-1620
FM | (MHz) | 87.5-108.0
Information system | RDS | - | RDS | -
Audio amplifier maximum output power | (W) | 25×4 (External type audio amplifier) | 25×4
Output impedance | (ohm) | 2 | 4
HDD | (GB) | 20 | -

### Speaker

Item | Specification
--- | ---
Door speaker | Tweeter | Woofer
Standard | BOSE
Front | Rear | Standard | BOSE | 4SD | 5HB, WGN
Maximum input | (W) | 25 | 100
Impedance | (ohm) | 4 | 2 | 4 | 3.2 | 0.5
Size | (in) | 5.5×7.5 | 6.5 | 5.25 | 2 | 9 | 5.25