#
PCM CONFIGURATION [L8, LF, L3]

id0140a5802600

1. Connect the WDS to DLC-2.

2. Set up the WDS (including the vehicle recognition.)

3. Select "Module programming."

4. Select "Programmable module installation."

5. Select "PCM" and perform procedures according to directions on the WDS screen.

  Note

  • If the PCM is replaced with a new one, the PCM stores DTC P0602 and illuminates the MIL even though no malfunction is detected. When the PCM CONFIGURATION is performed, then the stored DTC P0602 is deleted.

6. Retrieve DTC's by the WDS or equivalent, then verify that there in no DTC present.

  • If DTC is present, perform applicable DTC inspection.