#
ABS (ABS/TCS) HU/CM CONFIGURATION

id041300802600

1. Connect the WDS or equivalent to the DLC-2.

2. Input vehicle information following the directions on the WDS or equivalent screen.

3. Select "MODULE PROGRAMMING".

4. Select "PROGRAMMABLE MODULE INSTALLATION".

5. Select "ABS/TCS".

6. Retrieve DTCs using the WDS or equivalent, then verify that there is no DTC present.

  • If any DTC is present, perform applicable DTC inspection.