#
DTC TABLE [JA5AX-EL]

id050206800500

DTC No. | Condition | MIL | AT warning light | DC | *Monitor item | Memory function | Page
--- | --- | --- | --- | --- | --- | --- | ---
P0705 | Transaxle range (TR) switch circuit malfunction (power short circuit) | X | - | 2 | CCM | X | (See DTC P0705 [JA5AX-EL])
P0706 | Transaxle range (TR) switch circuit malfunction (open/ground short circuit) | X | - | 2 | CCM | X | (See DTC P0706 [JA5AX-EL])
P0711 | Transaxle fluid temperature (TFT) sensor malfunction (stuck) | X | - | 2 | CCM | X | (See DTC P0711 [JA5AX-EL])
P0712 | Transaxle fluid temperature (TFT) sensor circuit malfunction (short circuit) | X | X | 2 | CCM | X | (See DTC P0712 [JA5AX-EL])
P0713 | Transaxle fluid temperature (TFT) sensor circuit malfunction (open circuit) | X | X | 2 | CCM | X | (See DTC P0713 [JA5AX-EL])
P0715 | Input/turbine speed sensor circuit malfunction | X | X | 2 | CCM | X | (See DTC P0715 [JA5AX-EL])
P0720 | Vehicle speedometer sensor (VSS) circuit malfunction | X | X | 2 | CCM | X | (See DTC P0720 [JA5AX-EL])
P0740 | Torque converter clutch (TCC) system malfunction | X | - | 2 | CCM | X | (See DTC P0740 [JA5AX-EL])
P0743 | Torque converter clutch (TCC) solenoid valve circuit malfunction | X | X | 1 | CCM | X | (See DTC P0743 [JA5AX-EL])
P0748 | Pressure control solenoid circuit malfunction | - | X | - | CCM | X | (See DTC P0748 [JA5AX-EL])
P0751 | Shift solenoid A malfunction (stuck off) | X | - | 2 | CCM | X | (See DTC P0751 [JA5AX-EL])
P0752 | Shift solenoid A malfunction (stuck on) | X | - | 2 | CCM | X | (See DTC P0752 [JA5AX-EL])
P0753 | Shift solenoid A circuit malfunction (open/short) | X | X | 1 | CCM | X | (See DTC P0753 [JA5AX-EL])
P0756 | Shift solenoid B malfunction (stuck off) | X | - | 2 | CCM | X | (See DTC P0756 [JA5AX-EL])
P0757 | Shift solenoid B malfunction (stuck on) | X | - | 2 | CCM | X | (See DTC P0757 [JA5AX-EL])
P0758 | Shift solenoid B circuit malfunction (open/short) | X | X | 1 | CCM | X | (See DTC P0758 [JA5AX-EL])
P0761 | Shift solenoid C malfunction (stuck off) | X | - | 2 | CCM | X | (See DTC P0761 [JA5AX-EL])
P0762 | Shift solenoid C malfunction (stuck on) | X | - | 2 | CCM | X | (See DTC P0762 [JA5AX-EL])
P0763 | Shift solenoid C circuit malfunction (open/short) | X | X | 1 | CCM | X | (See DTC P0763 [JA5AX-EL])
P0768 | Reduction timing solenoid valve circuit malfunction (open/short) | - | X | - | CCM | X | (See DTC P0768 [JA5AX-EL])
P0773 | Neutral shift solenoid valve circuit malfunction (open/short) | - | X | - | CCM | X | (See DTC P0773 [JA5AX-EL])
P0778 | 2-4 brake solenoid valve circuit malfunction (open/short) | - | X | - | CCM | X | (See DTC P0778 [JA5AX-EL])
P0791 | Intermediate sensor circuit malfunction (open/short) | X | X | 2 | CCM | X | (See DTC P0791 [JA5AX-EL])
P0798 | High clutch solenoid valve circuit malfunction (open/short) | - | X | - | CCM | X | (See DTC P0798 [JA5AX-EL])
P1710 | GND return circuit malfunction | - | - | - | Other | X | (See DTC P1710 [JA5AX-EL])
U0073 | CAN BUS OFF | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM].)
U0100 | TCM cannot receive any signals from PCM | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM].)

  * :
Indicates the applicable item in On-Board System Readiness Test defined by CARB.