#
CONSOLE REMOVAL/INSTALLATION

id091700801200

Applied VIN (assumed):

JMZ GG12***# 100001-190206

JMZ GG14***# 100001-190206

JMZ GY19***# 100001-137241

JMZ GY89***# 100001-137241

1. For MT vehicle, remove the shift lever knob.

2. Slightly bend back the cradle. (with car-navigation system)

3. Remove the cup holder panel using a tape-wrapped screwdriver.

4. Remove the boot panel using a tape-wrapped screwdriver, disconnect the cigarette lighter connector, and remove the front ashtray illumination.

5. Remove the bolts.

6. Install in the reverse order of removal.

Applied VIN (assumed):

JMZ GG12***# 190207-

JMZ GG14***# 190207-

JMZ GY19***# 137242-

JMZ GY89***# 137242-

7. For MT vehicle, remove the shift lever knob.

8. Rotate the wiring harness clip installed on the cradle 90° in the direction indicated by the arrow in the figure and pull it out. (with car-navigation system)

9. Disconnect the cradle connector.

10. Remove the boot panel using a tape-wrapped screwdriver, disconnect the cigarette lighter connector, and remove the front ashtray illumination.

11. Remove the bolts.

12. Install in the reverse order of removal.