#
AUTOMATIC TRANSAXLE FLUID (ATF) REPLACEMENT [FS5A-EL]

id051721800600

  Warning

  • When the transaxle and ATF are hot, they can badly burn you. Turn off the engine and wait until they are cool before changing the ATF.

1. Remove the oil dipstick.

2. Remove the oil drain plug and washer.

3. Drain the ATF into a container.

4. Install a new washer and the drain plug.

Tightening torque

  29.4-41.2 N·m {3.0-4.2 kgf·m, 22-30 ft·lbf}

5. Add the specified ATF until ATF level reaches lower notch of dipstick type of ATF through the oil filler tube.

ATF type

  ATF M-V

Capacity (approx. quantity)

  Draining ATF from drain plug: 3.0 L {3.2 US qt, 2.4 lmp qt}
  Overhauling ATX: 5.0 L {5.3 US qt, 4.4 lmp qt}

6. Adjust the ATF amount to within the specified range according to the ATF inspection procedure. (See AUTOMATIC TRANSAXLE FLUID (ATF) INSPECTION [FS5A-EL].)

  Note

  • The full amount of ATF for the ATX is as follows

Capacity (approx. quantity)

  8.14 L {8.6 US qt, 7.2 lmp qt}