#
COMBINATION SWITCH REMOVAL/INSTALLATION

id091800469200

1. Disconnect the negative battery cable.

2. Remove the driver-side air bag module. (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

3. Remove the steering wheel. (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

4. Remove the column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

5. Remove the clock spring. (without DSC) (See CLOCK SPRING REMOVAL/INSTALLATION.)

  Caution

  • For vehicles with DSC, the clock spring is generally not to be removed from the combination switch as may result in a malfunction of the steering angle sensor. However, remove it only when replacing the clock spring as a single unit by referring to CLOCK SPRING REMOVAL/INSTALLATION. (See CLOCK SPRING REMOVAL/INSTALLATION.)

6. Remove in the order indicated in the table.

1 | Connector
2 | Screw
3 | Combination switch

7. Install in the reverse order of removal.