#
ON-BOARD DIAGNOSTIC SYSTEM PID/DATA MONITOR FUNCTION

id040200175200
• The PID/data monitor function is used for optionally selecting input/output signal monitor items preset in the ABS HU/CM or DSC HU/CM and reading them out in real-time.

## PID/DATA Monitor Table (Vehicles With ABS (ABS/TCS))

PID name | Input/output part | Operation/unit (WDS or equivalent)
--- | --- | ---
ABS_LAMP | ABS warning light driver output state | On/Off
ABSLF_I | LF ABS pressure retention valve output state | On/Off
ABSLF_O | LF ABS pressure reduction valve output state | On/Off
ABSLR_I | LR ABS pressure retention valve output state | On/Off
ABSLR_O | LR ABS pressure reduction valve output state | On/Off
ABSRF_I | RF ABS pressure retention valve output state | On/Off
ABSRF_O | RF ABS pressure reduction valve output state | On/Off
ABSRR_I | RR ABS pressure retention valve output state | On/Off
ABSRR_O | RR ABS pressure reduction valve output state | On/Off
ABSPMPRLY | ABS pump motor relay | On/Off
ABSVLVRLY | ABS valve control relay | On/Off
ABS_VOLT | System battery voltage value | V
BRAKE_LMP | BRAKE system warning light driver output state | On/Off
BOO_ABS | Brake pedal switch input | On/Off
CCNTABS | Number of continuous trouble code set | -
LF_WSPD | LF ABS wheel-speed sensor input | KPH, MPH
LR_WSPD | LR ABS wheel-speed sensor input | KPH, MPH
PCM_MSG | PCM | Present/Not Present
PMPSTAT | ABS pump motor states | On/Off
RF_WSPD | RF ABS wheel-speed sensor input | KPH, MPH
RPM | PCM | RPM
RR_WSPD | RR ABS wheel-speed sensor input | KPH, MPH
TCM_MSG* | TCM | Present/Not Present

  * :
Only vehicles with ATX

## PID/DATA Monitor Table (Vehicles With DSC)

PID name | Input/output part | Operation/unit (WDS or equivalent)
--- | --- | ---
ABS_LAMP | ABS warning light driver output state | On/Off
ABSLF_I | LF ABS pressure retention valve output state | On/Off
ABSLF_O | LF ABS pressure reduction valve output state | On/Off
ABSLR_I | LR ABS pressure retention valve output state | On/Off
ABSLR_O | LR ABS pressure reduction valve output state | On/Off
ABSRF_I | RF ABS pressure retention valve output state | On/Off
ABSRF_O | RF ABS pressure reduction valve output state | On/Off
ABSRR_I | RR ABS pressure retention valve output state | On/Off
ABSRR_O | RR ABS pressure reduction valve output state | On/Off
ABSPMPRLY | ABS pump motor relay | On/Off
ABSVLVRLY | ABS valve control relay | On/Off
ABS_VOLT | System battery voltage value | V
ACCLMTR*1 | Combined sensor (forward-G sensor) | G
AWD_MSG*1 | 4WD control module | Present/Not Present
BOO _ABS | Brake pedal switch input | On/Off
BRK_FLUID | Brake fluid level sensor input | OK/Low
BRAKE_LMP | BRAKE system warning light driver output state | On/Off
CCNTABS | Number of continuous trouble code set | -
IC_MSG | Instrument cluster | Present/Not Present
LAT_ACCL | Combined sensor (Lateral-G sensor) | G
L_DSC_O | Stability control solenoid valve (LF-RR) | On/Off
LF_WSPD | LF ABS wheel-speed sensor input | KPH, MPH
LR_WSPD | LR ABS wheel-speed sensor input | KPH, MPH
MCYLI P | Brake fluid pressure sensor | Pa
PCM_MSG | PCM | Present/Not Present
PMPSTAT | ABS pump motor states | On/Off
R_DSC_O | Stability control solenoid valve (RF-LR) | On/Off
RF_WSPD | RF ABS wheel-speed sensor input | KPH, MPH
RPM | PCM | RPM
RR_WSPD | RR ABS wheel-speed sensor input | KPH, MPH
SWA_POS | Steering angle sensor | °
TCM_MSG*2 | TCM | Present/Not Present
TC LVAL | Traction switch solenoid valve (LF-RR) | On/Off
TC RVAL | Traction switch solenoid valve (RF-LR) | On/Off
TPI | PCM | %
TRAC_SW*3 | DSC OFF switch | On/Off
TRANSGR | PCM (MTX) or TCM (ATX) | 1/2/3/4/5/6/R/N/Error
YAW_RATE | Combined sensor (yaw rate sensor) | °/s

  *1 :
Only vehicles with 4WD
  *2 :
Only vehicles with ATX
  *3 :
Only vehicles with L3 Turbo