#
4WD CONTROL MODULE REMOVAL/INSTALLATION [L3 Turbo]

id0318a2806000

## L.H.D.

1. Disconnect the negative battery cable.

2. Remove the lower panel.

3. Remove in the order indicated in the table.

1 | Connector
2 | Nut
3 | 4WD CM

4. Install in the reverse order of removal.

## R.H.D.

1. Remove in the order indicated in the table.

1 | PCM cover No.1 (See PCM REMOVAL/INSTALLATION [L3 Turbo])
2 | Connector
3 | Nut
4 | 4WD CM

2. Install in the reverse order of removal.