#
TRANSFER OIL SEAL REPLACEMENT [A26MX-R]

id0316d3800400

1. On level ground, jack up the vehicle and support it evenly on safety stands.

2. Drain the oil from the transfer. (See TRANSFER OIL REPLACEMENT [A26MX-R].)

3. Remove the joint shaft. (See JOINT SHAFT REMOVAL/INSTALLATION [L3 Turbo])

4. Remove the oil seals using a screwdriver.

5. Using the SST and a hammer, tap each new oil seal.

6. Coat the lip of each oil seal with transfer oil.

7. Install the joint shaft. (See JOINT SHAFT REMOVAL/INSTALLATION [L3 Turbo])

8. Add the specified amount and type of oil. (See TRANSFER OIL REPLACEMENT [A26MX-R].)