#
5TH/6TH GEAR THRUST CLEARANCE PREINSPECTION

id051500810100

1. Remove the rear cover.

2. Measure the 5th gear thrust clearance using a feeler gauge.

  • If it exceeds the maximum specification, inspect the contact surfaces of 5th gear and the clutch hub. Replace worn or damaged parts.

5th gear thrust clearance

  Standard: 0.100-0.220 mm {0.0040-0.0086 in}
  Maximum: 0.270 mm {0.0106 in}

3. Measure the 6th gear thrust clearance using a dial indicator.

  • If it exceeds the maximum specification, inspect the contact surfaces of 6th gear and the clutch hub. Replace worn or damaged parts.

6th gear thrust clearance

  Standard: 0.100-0.220 mm {0.0040-0.0086 in}
  Maximum: 0.270 mm {0.0106 in}