#
CAMSHAFT OIL CLEARANCE INSPECTION [WITH DIESEL PARTICULATE FILTER]

id0110f3501600

1. Position plastigage atop the journals in the axial direction.

2. Install the camshaft cap and rocker arm shaft. (See Rocker Arm and Rocker Arm Shaft Assembly Note)

3. Remove the camshaft cap and rocker arm shaft. (See Rocker Arm and Rocker Arm Shaft Disassembly Note)

4. Measure the oil clearance. Replace the cylinder head if necessary.

Standard clearance

  0.025-0.075 mm {0.001-0.003 in}

Maximum clearance

  0.105 mm {0.004 in}