#
TRANSFER OIL INSPECTION [A26MX-R]

id0316d3800200

1. Park the vehicle on level ground.

2. Remove the oil level plug and with the washer.

3. Verify that the oil is near the brim of the plug port.

  • If the oil level is low, add the specified amount and type of oil through the oil level plug hole.

Transfer oil [A26MX-R]

  Specified oil grade: API Service GL-5
  Specified oil viscosity: SAE 80W-90

4. Tighten the oil level plug with a new washer.

Tightening torque

  39.2-58.8 N·m {4.0-5.9 kgf·m, 29.0-43.3 ft·lbf}