#
COOLING FAN MOTOR REMOVAL/INSTALLATION [L8, LF, L3]

id0112b28019b1

  Warning

  • Remove and install all parts when the engine is cold, otherwise they can cause severe burns or serious injury.

  Note

  • There are three types of cooling fan components, A, B, and C. Types A, B, and C can be identified from the number of blades on the cooling fans No. 1 and No. 2. Refer to the following table to identify the cooling fan type.

Cooling fan components | Number of blades
--- | ---
Cooling fan No.1 (LH) | Cooling fan No.2 (RH)
Type A | 5 | 7
Type B | 7 | 5
Type C | 7 | 4

1. Disconnect the negative battery cable.

2. Remove the shroud panel. (See SHROUD PANEL REMOVAL/INSTALLATION.)

3. Remove the cooler pipe stay. (See CONDENSER REMOVAL/INSTALLATION.)

4. Remove the ATX oil cooler hose stay. (ATX) (See OIL COOLER REMOVAL/INSTALLATION [JA5AX-EL].)

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

.

1 | Cooling fan motor connectors
2 | Wiring harness
3 | Coolant reserve tank hose
4 | Cooling fan component
5 | Cooling fan No.1
6 | Cooling fan No.2
7 | Cooling fan motor No.1
8 | Cooling fan motor No.2