#
OIL COOLER REMOVAL/INSTALLATION [JA5AX-EL]

id051705801600

1. Disconnect the negative battery cable.

2. Drain the ATF into a container. (See AUTOMATIC TRANSAXLE FLUID (ATF) REPLACEMENT [JA5AX-EL].)

3. Remove the radiator. (See RADIATOR REMOVAL/INSTALLATION [L8, LF, L3].)

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

6. Add ATF to the specified level. (See AUTOMATIC TRANSAXLE FLUID (ATF) REPLACEMENT [JA5AX-EL].)

7. Connect the negative battery cable.

8. Inspect for oil leakage from the oil pipes and oil hoses.

9. Inspect for coolant from the hoses.

10. Inspect the ATF level and condition. (See AUTOMATIC TRANSAXLE FLUID (ATF) INSPECTION [JA5AX-EL].)

11. Carry out the line pressure test. (See MECHANICAL SYSTEM TEST [JA5AX-EL].)

12. Carry out the road test. (See ROAD TEST [JA5AX-EL].)

.

1 | Oil hose (See Oil Pipe, Hose Clamp, Oil Hose Installation Note)
2 | Hose clamp (See Oil Pipe, Hose Clamp, Oil Hose Installation Note)
3 | Oil cooler
4 | Oil pipe (See Oil Pipe, Hose Clamp, Oil Hose Installation Note)
5 | Radiator (in tank oil cooler) (See Radiator (In Tank Oil Cooler) Installation Note)

## Radiator (In Tank Oil Cooler) Installation Note

1. The automatic transaxle oil cooler flushing must be performed whenever a transaxle is removed for service because the existing fluid may be contaminated, and to prevent contamination of new fluid.

  Note

  • The flushing must be performed after installation of the overhauled or replacing transaxle.

2. Follow the instructions in the manufacturer's publication for flushing operation.

## Oil Pipe, Hose Clamp, Oil Hose Installation Note

1. Apply compressed air to cooler-side opening, and blow any remaining grime and foreign material from the cooler pipes. Compressed air should be applied for no less than one minute.

2. Align the marks, and slide the oil hose onto the oil pipe until it is fully seated as shown.

  Note

  • If reusing the hose, install the new hose clamp exactly on the mark left by the previous hose camp.Then apply force to the hose clamp in the direction of the arrow in order to fit the clamp in the place.

3. Install the new hose clamp onto the hose.

4. Verify that the hose clamp does not interfere with any other components.