#
DOOR ADJUSTMENT

id091100800400

1. Measure the gap and height between the front or rear door and the body.

2. If there is any malfunction, loosen the front or rear door hinge installation bolts or the door lock striker installation screws, and reposition the door.

Clearance

  a: 2.5-4.5 mm {0.10-0.18 in}
  b: -0.8-1.2 mm {-0.03-0.05 in}
  c: -0.3-1.7 mm {-0.01-0.07 in}
  d: -1.0-1.0 mm {-0.04-0.04 in}
  e: -0.5-1.5 mm {-0.02-0.06 in}

3. Tighten the bolts or screws.