#
REAR WASHER HOSE REMOVAL/INSTALLATION [5HB]

id0919004757a3

1. Disconnect the negative battery cable.

2. Remove the washer tank. (See WASHER TANK REMOVAL/INSTALLATION.)

3. Partially peel off the right side mud guard.

4. Remove rear washer hose No.1 from the clips.

5. Remove rear washer hose No.1 and joint pipe A.

6. Remove the A-pillar trim. (See A-PILLAR TRIM REMOVAL.)

7. Remove rear washer hose No.2 from clip A.

8. Remove clips B from the body.

9. Remove rear washer hose No.2 and joint pipes B.

10. Remove the c-pillar trim. (See C-PILLAR TRIM REMOVAL/INSTALLATION [4SD, 5HB].)

11. Remove the liftgate upper trim. (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION [5HB].)

12. Remove rear washer hose No.3 from clip C.

13. Remove clips D from the body.

14. Remove rear washer hose No.3 and joint pipe C.

15. Remove the headliner. (See HEADLINER REMOVAL/INSTALLATION [4SD, 5HB].)

16. Remove the tape from rear washer hose No.4.

17. Install in the reverse order of removal.