#
CAMSHAFT POSITION (CMP) SENSOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

id0140f1801500

  Caution

  • When foreign material, such as iron chips, gets on the CMP sensor, it can cause abnormal output from the sensor because of flux turbulence and adversely affect engine control. Be sure there is no foreign material on the CMP sensor when replacing.
  • Do not forcefully pull the wiring harness of the CMP sensor. Doing so will break the harness.

1. Disconnect the negative battery cable.

2. Remove the engine cover.

3. Remove in the order indicated in the table.

1 | CMP sensor installation bolt
2 | CMP sensor (See CMP Sensor Installation Note)

4. Verify that the O-ring is not damaged.

  • If there is a damage, replace the CMP sensor.

5. Apply a small amount of clean oil to the O-ring and the head cover.

6. Install in the reverse order of removal.

## CMP Sensor Installation Note

1. Verify that there is no foreign material on the CMP sensor flange surface and the installation surface.

2. Press in the CMP sensor until the CMP sensor flange surface firmly adheres to the installation surface.

3. Verify that the O-ring is installed correctly to the sensor installation hole.

4. Tighten the bolt.