#
FAN CONTROL MODULE CONSTRUCTION/OPERATION [L3 Turbo]

id0112b21006b3

## Construction

• Fan control module is installed on the radiator cowling.
• Fan control module cannot be separated from cooling fan motor No.1 because they are integrated.

1 | Fan control module
2 | Radiator cowling
3 | Cooling fan motor No.1

## Operation

• The fan control module drives the both fan motors based on the cooling fan control signal sent by the PCM according to the following:

  - Engine coolant temperature
  - Vehicle speed
  - Whether A/C middle pressure switch is on or off
  - Whether the A/C magnetic clutch is on or off

• The fan control module allows continuously variable control of the fan motor rotation rate reducing fan operation noise and power consumption.

1 | Cooling fan electrical system wiring diagram
2 | Battery
3 | Fan control module
4 | Cooling fan motor No.1
5 | Cooling fan motor No.2

## Fail-safe function

1. Over-heat fail-safe

  - If the internal area of the fan control module exceeds the specified temperature, the fan control module fixes the output duty value to the set value.
  - If the internal area of the fan control module returns to the specified temperature, the fan control module returns to normal control.

2. Input signal open circuit fail-safe

  - If there is an open circuit in the wiring harness between the PCM and the fan control module, the fan control module fixes the output duty value to the set value.