#
CYLINDER HEAD COVER CONSTRUCTION [L8, LF, L3]

id0110a1100200
• The cylinder head cover is made of integrated plastic, which is lightweight and sound absorbent.
• The oil filler cap is a bayonet type. The boss for installing the camshaft position (CMP) sensor is provided at the rear of the cylinder head cover.
• LF and L3 engine models has a hole for installing the oil control valve (OCV).
• A dipstick insertion hole has been equipped to the cylinder head cover.

1 | Camshaft position (CMP) sensor attachment part
2 | Oil control valve (OCV) attachment hole (LF, L3)
3 | Dipstick insertion hole