#
DOOR GARNISH INSTALLATION

id091600801400

1. Remove the adhesive remaining on the side protector (if it will be reused) and the body using a razor.

2. Remove any grease or dirt from the adhesion surface of the side protector (if it will be reused) and the body.

3. Attach double-sided adhesive tape to the side protector as shown (if it will be reused).

4. Peel off the backing of the double-sided adhesive tape and attach the door garnish onto the body.