#
POWER STEERING PRESSURE (PSP) SWITCH CONSTRUCTION/OPERATION [MZR-CD (RF Turbo)]

id0140f1174600
• Installed to the power steering oil pump.

1 | PSP switch
2 | Power steering oil pump

• While the power steering is operating, the power steering oil pump turns on when the hydraulic pressure in the power steering oil pump reaches the PSP switch activation pressure, and turns off when the hydraulic pressure lowers to a certain value from the PSP switch activation pressure.