#
PRE-DELIVERY INSPECTION

id000000801100

## Pre-Delivery Inspection Table

### Exterior

INSPECT and ADJUST, if necessary, the following items to specification:

□Glass, exterior bright metal and paint for damage

□All weatherstrips for damage or detachment

□Door operation and alignment including side door and back door

□Wheel lug nuts

□Tire pressures

□Headlight aiming

□Headlight cleaner and fluid level (if equipped)

□Operation of bonnet release and lock

□Operation of fuel lid opener

INSTALL the following parts:

□Flap (front and rear)

□Wheel caps or rings (if equipped)

### Under Bonnet-Engine Off

INSPECT and ADJUST, if necessary, the following items to specification:

□Fuel, engine coolant, and hydraulic lines, fittings, connections, and components for leaks

□Tension of drive belts

□Tightness of water hose clamps

□Tightness of battery terminals, electrolyte level and specific gravity

□Radiator coolant level and specific gravity

□Engine oil level

□Oil level in steering gearbox

□Windshield washer tank fluid level

□Brake master cylinder fluid level

□Clutch master cylinder fluid level

□Power steering fluid level

□Automatic transaxle fluid level

CLEAN the spark plugs

### Interior

INSTALL the following parts:

□Fuse for accessories

□Equipments for advanced keyless system (if equipped)

  • After install the accessories fuse, assemble the card key (transmitter and auxiliary key)
  • Install the start knob to the ignition switch

CHECK the operations of the following items:

□All lights including warning, and indicator lights

□Cigarette lighter and clock

□Ignition switch and steering lock

□Transaxle range switch

□Warning buzzers

□Seat belts warning system

□Ignition key reminder alarm

□Seat controls (sliding and reclining) and headrests

□Door locks, including childproof door locks

□Power door lock

□Power windows (if equipped)

□Horn, wipers, and washers

□Wiper blades performance

Clean the wiper blades and windshield, if necessary

□Antenna

CHECK the following items:

□Presence of spare fuse

□Upholstery and interior finish

CHECK and ADJUST, if necessary, the following items:

□Operation and fit of windows

□Parking brake

□Pedal height and free play of brake pedal

### Under Bonnet-Engine Running at Operating Temperature

CHECK the following items:

□Operation of idle-up system for electrical load, air conditioner

□Idle speed

□Automatic transaxle fluid

□Initial ignition timing

□Operation of throttle position sensor

□Operation of EGR valve (if equipped)

### On Hoist

CHECK the following items:

□Underside fuel, coolant and hydraulic lines, fittings, connections, and components for leaks

□Tires for cuts or bruises

□Steering linkage, suspension, exhaust system, and all underside hardware for looseness or damage

□Manual transaxle oil level

### Road Test

CHECK the following items:

□Brake operation

□Clutch operation

□Steering control

□Operation of meters and gauges, squeaks, rattles, and abnormal noises

□Engine general performance

□Emergency locking retractors

### After Road Test

REMOVE the seat and floor mat protective covers

CHECK for the necessary owner information materials, tools, and spare tire in vehicle