#
POWER OUTSIDE MIRROR DISASSEMBLY/ASSEMBLY [TYPE A]

id0912008075b3

1. Disassemble in the order indicated in the table.

1 | Outside mirror glass (See Outside Mirror Glass Disassembly Note.) (See Outside Mirror Glass Assembly Note.)
2 | Connector (vehicles with heated outside mirror)
3 | Cover (See Cover Disassembly Note.)
4 | Outside mirror holder

2. Assemble in the reverse order of disassembly.

## Outside Mirror Glass Disassembly Note

1. Press area A of the glass so that area B moves toward you.

2. Insert a flathead screwdriver into the notch and remove the glass from the mirror base.

## Cover Disassembly Note

1. Pull off the mirror holder tab with a flathead screwdriver and press the mirror cover tab downward.

## Outside Mirror Glass Assembly Note

1. Press the mirror into the base so that the pin does not dislodge.