#
REAR BUMPER DISASSEMBLY/ASSEMBLY [L3 TURBO]

id0910004056a1

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

1 | Bumper guard (See Bumper Guard Removal Note)
2 | Reflector (See Reflector Removal Note)
3 | Pipe garnish
4 | Rear bumper fascia

## Bumper Guard Removal Note

1. Detach tabs C and remove the bumper guard.

## Reflector Removal Note

1. Lift the reflector up in the direction of the arrow, then unhook it from the rear bumper.