#
CARGO COMPARTMENT LIGHT REMOVAL/INSTALLATION [WGN]

id0918004663a6

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Lens (See Lens Removal Note.)
2 | Cargo compartment light bulb
3 | Screw (if equipped)
4 | Cargo compartment light
5 | Connector

3. Install in the reverse order of removal.

## Lens Removal Note

1. Insert a tape-wrapped flathead screwdriver into the service hole.

2. Twist the flathead screwdriver as indicated by the arrow to remove the lens.