#
KEYLESS ENTRY SYSTEM OUTLINE [ADVANCED KEYLESS SYSTEM]

id0914b51014b1
• An advanced keyless system has been adopted that enables the driver to start the engine or lock/unlock the doors without operating the key or transmitter (card key) by carrying the card key that has been programmed to the vehicle.
• The doors also can be locked/unlocked by operating the key (sub-key) or transmitter (card key).
• The answer-back function has been adopted where the hazard warning light flashes and a buzzer sounds to confirm that the doors are locked/unlocked. Also, the advanced keyless entry system indicates activation by a buzzer sound.
• A warning and guidance function has been adopted that promotes correction if the system is operated impropeLRy, and uses the indicator light in the instrument cluster, a buzzer sound, and the keyless buzzer from the driver's side front fender panel.
• A customize function that switches the activation/deactivation of each function has been adopted.
• A rolling code type transmitter (card key) has been adopted to prevent theft by radiowave interception.
• To prevent improper operation while the vehicle is moving, the doors cannot be locked/unlocked by operating the transmitter (card key) or request switch if the start knob is not in the LOCK position.