#
NEUTRAL SWITCH CONSTRUCTION/OPERATION [L3 Turbo]

id0140b6176900
• When the shift lever is in the neutral position, the contact closes (ON) and the PCM detects a voltage of 0 V. When the shift lever is not in the neutral position, the contact opens (OFF) and the PCM detects a voltage of 12 V.

.

1 | Neutral switch
2 | Push ON
3 | Other then neutral (OFF)
4 | Neutral (ON)
5 | Neutral (ON)
6 | Except above
7 | No load
8 | Load