#
FRONT MAP LIGHT REMOVAL/INSTALLATION

id091800808000

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Front map light (See Front Map Light Removal Note.)
2 | Connector
3 | Socket
4 | Map light bulb

3. Install in the reverse order of removal.

## Front Map Light Removal Note

1. Insert a tape-wrapped flathead screwdriver into the gap between the headliner and the front map light.

2. Push the hooks to remove the front map light.