#
DTC P0113 [MZR-CD (RF Turbo)]

id0102f1803800

DTC P0113 | Intake air temperature (IAT) sensor No.1 circuit high input
--- | ---
DETECTION CONDITION | • The PCM monitors the input signal from the IAT sensor No.1. If the voltage from the IAT sensor No.1 is more than 4.9 V, the PCM determines that there is a malfunction in the IAT sensor No.1 circuit. Diagnostic support note • The MIL illuminates if the PCM detects the above malfunction condition in the first drive cycle. • FREEZE FRAME DATA is available. • The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • IAT sensor No.1 malfunction • Connector or terminal malfunction • Open circuit in wiring harness between MAF/IAT sensor terminal D and PCM terminal 55 • Short to power supply in wiring harness between MAF/IAT sensor terminal D and PCM terminal 55 • Open circuit in wiring harness between MAF/IAT sensor terminal E and PCM terminal 78 • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY CURRENT SIGNAL STATUS: IS CONCERN INTERMITTENT OR CONSTANT? • Connect the WDS or equivalent to the DLC-2. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Go to the next step.
No | Intermittent concern exists. Perform the "INTERMITTENT CONCERN TROUBLESHOOTING". (See INTERMITTENT CONCERN TROUBLESHOOTING [MZR-CD (RF Turbo)].)
4 | INSPECT MAF/IAT SENSOR CONNECTOR FOR POOR CONNECTION • Turn the engine switch off. • Disconnect the MAF/IAT sensor connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 9.
No | Go to the next step.
5 | INSPECT IAT SENSOR NO.1 SIGNAL CIRCUIT FOR SHORT TO POWER SUPPLY • Turn the engine switch to the ON position (Engine off). • Measure the voltage between MAF/IAT sensor terminal D (wiring harness-side) and body ground. • Is the voltage more than 4.9 V? | Yes | Repair or replace the wiring harness for a possible short to power supply, then go to Step 9.
No | Go to the next step.
6 | INSPECT IAT SENSOR NO.1 • Inspect the IAT sensor No.1. (See INTAKE AIR TEMPERATURE (IAT) SENSOR INSPECTION [MZR-CD (RF Turbo)].) • Is there any malfunction? | Yes | Replace the MAF/IAT sensor, then go to Step 9. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to the next step.
7 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn the engine switch off. • Disconnect the PCM connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 9.
No | Go to the next step.
8 | INSPECT IAT SENSOR NO.1 CIRCUIT FOR OPEN CIRCUIT • Turn the engine switch off. • Inspect for continuity between the following terminals: - MAF/IAT sensor terminal D (wiring harness-side) and PCM terminal 55 (wiring harness-side) - MAF/IAT sensor terminal E (wiring harness-side) and PCM terminal 78 (wiring harness-side) • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for a possible open circuit, then go to the next step.
9 | VERIFY TROUBLESHOOTING OF DTC P0113 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to the next step.
10 | VERIFY AFTER REPAIR PROCEDURE • Perform the Repair Verification Drive Mode. (See OBD DRIVE MODE [MZR-CD (RF Turbo)].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | DTC troubleshooting completed.