#
THERMOSTAT INSPECTION [MZR-CD (RF Turbo)]

id0112f1801300

1. Inspect the thermostat for the following.

  Warning

  • During inspection, the thermostat and water are extremely hot and they can cause burns. Do not touch the thermostat and water.

  • The valve should not open under normal temperature.
  • Opening temperature and valve lift

  - If there is malfunction, replace the thermostat.

Thermostat initial-opening temperature

  80-84 °C {176-183 °F}

Thermostat full-open temperature

  95 °C {203 °F}

Thermostat full-open lift

  More than 8.5 mm {0.33 in}