#
CLUTCH HOUSING AND TRANSAXLE CASE COMPONENTS DISASSEMBLY [TYPE A]

id051500803712

1. Disassemble in the order indicated in the table.

1 | Bearing race (primary shaft)
2 | Oil seal (primary shaft) (See Oil Seal (Primary Shaft) Disassembly Note.)
3 | Bearing race (secondary shaft) (See Bearing Race (Secondary Shaft) Disassembly Note.)
4 | Funnel
5 | Guide plate
6 | Sealing cap (See Sealing Cap Disassembly Note.)
7 | Roll pin (See Roll Pin Disassembly Note.)
8 | Roll pin (See Roll Pin Disassembly Note.)
9 | Control rod
10 | Selector
11 | Change arm
12 | Breather cover component
13 | Breather
14 | Hole cover
15 | Oil seal (differential) (See Oil Seal (Differential) Disassembly Note.)
16 | Bearing race (differential) (See Bearing Race (Differential) Disassembly Note.)
17 | Inner shift lever
18 | Push pin component and spring
19 | Drain plug and washer
20 | Bearing race (transaxle case) (See Bearing Race (Transaxle Case) Disassembly Note.)
21 | Adjustment shim
22 | Bearing race (differential) (See Bearing Race (Differential) Disassembly Note.)
23 | Adjustment shim
24 | Oil seal (differential) (See Oil Seal (Differential) Disassembly Note.)
25 | Roll pin
26 | Shift lever component
27 | Key
28 | Control end
29 | Spring and washer
30 | Shift lever shaft
31 | Boots
32 | Oil passage

## Oil Seal (Primary Shaft) Disassembly Note

1. Remove the oil seal using a flathead screwdriver.

## Bearing Race (Secondary Shaft) Disassembly Note

1. Remove the bearing race by lifting it and the funnel out together.

## Sealing Cap Disassembly Note

1. Move the control rod in the direction of the arrow.

2. Using a flathead screwdriver and hammer, make a hole on the cap.

3. Remove the seal cap by putting the flathead screwdriver into the hole, made in Step 2, from the inside of the transaxle.

## Roll Pin Disassembly Note

1. Align the groove for removal of the clutch housing pin with the position of the roll pin, then tap the pin out using a pin punch.

## Oil Seal (Differential) Disassembly Note

1. Remove the oil seal using a flathead screwdriver.

## Bearing Race (Differential) Disassembly Note

1. Remove the bearing outer race using the SST.

## Bearing Race (Transaxle Case) Disassembly Note

1. Remove the bearing race using the SST.