#
REAR WASHER HOSE REMOVAL/INSTALLATION [WGN]

id0919004757a4

1. Disconnect the negative battery cable.

2. Remove the washer tank.

3. Partially peel off the right side mud guard.

4. Remove rear washer hose No.1 from the clips.

5. Remove rear washer hose No.1 and joint pipe A.

6. Remove joint pipe C from the body.

7. Remove the A-pillar trim.

8. Remove rear washer hose No.2 from clip A.

9. Remove clips B from the body.

10. Remove rear washer hose No.2 and joint pipes B.

11. Remove the D-pillar trim.

12. Remove the liftgate upper trim. (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION [WGN].)

13. Remove rear washer hose No.3 from clip C.

14. Remove rear washer hose No.3 and joint pipe D.

15. Remove the headliner. (See HEADLINER REMOVAL/INSTALLATION [WGN].)

16. Remove the tape from rear washer hose No.4.

17. Install in the reverse order of removal.