#
DTC B2777, B2778, B2779, B2780

id080200803000

DTC | B2777 | Passenger-side curtain air bag module circuit resistance low
--- | --- | ---
B2778 | Passenger-side curtain air bag module circuit resistance high
B2779 | Passenger-side curtain air bag module circuit short to body ground
B2780 | Passenger-side curtain air bag module circuit short to power supply
DETECTION CONDITION | Warning • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection according to only the detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the inspection procedure. • Resistance other than 1.3-4.7 ohms detected in passenger-side curtain air bag module circuit • Malfunction in wiring harness between passenger-side curtain air bag module and SAS control module
POSSIBLE CAUSE | • Open or short circuit in wiring harness between passenger-side curtain air bag module and SAS control module • Passenger-side curtain air bag module malfunction • SAS control module malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT PASSENGER-SIDE CURTAIN AIR BAG MODULE • Using the WDS or equivalent, verify the following PID/DATA monitor. (See PID/DATA MONITOR TABLE.) - PS_CURT_ST • Is the resistance of the passenger-side curtain air bag module normal? - Resistance: 1.3-4.7 ohms | Yes | Replace the SAS control module. (See SAS CONTROL MODULE REMOVAL/INSTALLATION.)
No | Go to the next step.
2 | INSPECT PASSENGER-SIDE CURTAIN AIR BAG MODULE CONNECTOR Warning • Handling the air bag system components improperly can accidentally deploy the air bag modules and pre-tensioner seat belts, which may seriously injure you. Read the service warnings and cautions before handling the air bag system components. (See SERVICE WARNINGS.) (See SERVICE CAUTIONS.) • Turn the ignition switch to the LOCK position. • Disconnect the negative battery cable and wait for 1 min or more. • Remove the C-pillar trim. (See C-PILLAR TRIM REMOVAL/INSTALLATION [4SD, 5HB].) (See C-PILLAR TRIM REMOVAL/INSTALLATION [WGN].) • Disconnect the passenger-side curtain air bag module connector. • Is there any malfunction of the passenger-side curtain air bag module connector? | Yes | Replace the air bag wiring harness.
No | Go to the next step.
3 | VERIFY WHETHER MALFUNCTION IS IN PASSENGER-SIDE CURTAIN AIR BAG MODULE OR RELATED WIRING HARNESS • Connect the leads of the SST (Fuel and thermometer checker) or apply 2-ohm resistance to passenger-side curtain air bag module connector terminals A and B. • Set the resistance of the SST (Fuel and thermometer checker) to the 2-ohm position. • Connect the negative battery cable. • Turn the ignition switch to the ON position. • Are DTCs B2777, B2778, B2779 and/or B2780 indicated? | Yes | Go to the next step.
No | Replace the passenger-side curtain air bag module. (See CURTAIN AIR BAG MODULE REMOVAL/INSTALLATION.)
4 | INSPECT WIRING HARNESS BETWEEN PASSENGER-SIDE CURTAIN AIR BAG MODULE AND SAS CONTROL MODULE • Turn the ignition switch to the LOCK position. • Disconnect the negative battery cable and wait for 1 min or more. • Disconnect the driver and passenger-side front seat connectors. • Disconnect the driver and passenger-side curtain air bag module connectors. • Turn up floor covering. • Inspect the wiring harness between SAS control module terminal 2D and passenger-side curtain air bag module terminal A, SAS control module terminal 2A and passenger-side curtain air bag module terminal B for the following: - Short to ground - Short to power supply - Open circuit • Is the wiring harness normal? | Yes | Replace the SAS control module. (See SAS CONTROL MODULE REMOVAL/INSTALLATION.)
No | Replace the air bag wiring harness.