#
STEERING TECHNICAL DATA

id065000800200

Item | Specification
--- | ---
Power steering fluid type | ATF M-III or equivalent (e.g. Dexron®II)
Power steering fluid capacity (approximate quantity) | 2WD MTX (L8, LF, L3 (except 18inch wheel)): 0.80 L {0.84 US qt, 0.70 Imp qt} 2WD MTX (L3 (18 inch wheel)): 0.82 L {0.87 US qt, 0.72 Imp qt} 2WD ATX (LF, L3 (except 18inch wheel)): 0.87 L {0.92 US qt, 0.77 Imp qt} 2WD ATX (L3 (18 inch wheel)): 0.89 L {0.94 US qt, 0.78 Imp qt} 4WD (L3, L3 Turbo): 0.89 L {0.94 US qt, 0.78 Imp qt} MZR-CD (RF Turbo): 0.86 L {0.91 US qt, 0.76 Imp qt}
Steering wheel play | 0-30 mm {0-1.18 in}
Steering wheel effort | 7.8 N·m {80 kgf·cm, 58 in·lbf} max.
Steering shaft length | 211.6 mm {8.3 in}
Steering rack runout | Large diameter portion: 0.15 mm {0.006 in} max. Small diameter portion: 0.20 mm {0.008 in} max.
Tie-rod end rotational torque | 0.6-2.0 N·m {6.2-20.3 kgf·cm, 5.4-17.7 in·lbf} [Pull scale reading 6.0-20.0 N {0.62-2.03 kgf, 1.4-4.4 lbf}]
Tie rod swing torque | 0.4-4.0 N·m {4.1-40.7 kgf·cm, 3.6-35.4 in·lbf} [Pull scale reading 4.0-40.0 N {0.41-4.07 kgf, 0.9-8.9 lbf}]
Pinion shaft rotation torque | Center of rack ±90°: 0.7-1.1 N·m {7.2-11.2 kgf·cm, 6.2-9.7 in·lbf} Except center of rack ±90°: Less than 1.6 N·m {16.3 kgf·cm, 11.8 in·lbf}

Oil pump fluid pressure

Type | Oil pump fluid pressure (MPa {kgf/cm2, psi})
--- | ---
2WD (L8, LF, L3 (except 18 inch wheel)) | 10.80-11.29 {110.2-115.1, 1,567-1637}
2WD (MZR-CD (RF Turbo)) | 11.31-11.80 {115.4-120.3, 1,641-1,711}
4WD (L3), 2WD (18 inch wheel) | 10.30-10.79 {105.1-110.0, 1,490-1,564}
4WD (L3 Turbo) | 11.30-11.70 {116.0-119.0, 1,639-1,696}

Gear housing fluid pressure

Type | Oil pump fluid pressure (MPa {kgf/cm2, psi})
--- | ---
2WD (L8, LF, L3 (except 18 inch wheel)) | 10.80-11.29 {110.2-115.1, 1,567-1637}
2WD (MZR-CD (RF Turbo)) | 11.31-11.80 {115.4-120.3, 1,641-1,711}
4WD (L3), 2WD (18 inch wheel) | 10.30-10.79 {105.1-110.0, 1,490-1,564}
4WD (L3 Turbo) | 11.30-11.70 {116.0-119.0, 1,639-1,696}