#
INBOARD COMBINATION LIGHT REMOVAL/INSTALLATION

id091800810700

1. Disconnect the negative battery cable.

2. Remove the trunk lid trim (liftgate lower trim). (See TRUNK LID TRIM REMOVAL/INSTALLATION.) (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION [5HB].) (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION [WGN].)

3. Remove in the order indicated in the table.

1 | Connector
2 | Nut
3 | Inboard combination light (See Inboard Combination Light Installation Note.)
4 | Socket
5 | Back-up light bulb
6 | Rear fog light bulb (L.H.D.: left side only, R.H.D.: right side only)

4. Install in the reverse order of removal.

## Inboard Combination Light Installation Note

1. Insert the inboard combination light into the trunk lid (liftgate) as shown in the figure, then pivot it inward and fix in place.

2. Place the bracket in the proper position as shown in the figure and press it to the trunk lid (liftgate) to attach.