#
IMMOBILIZER SYSTEM OUTLINE [WITHOUT ADVANCED KEYLESS SYSTEM]

id0914b31017b6
• A passive anti-theft system (PATS), which incorporates the former immobilizer unit function, has been adopted and is built-into the PCM.
• The PATS prevents vehicle theft by only allowing keys that have been registered specifically for the vehicle to start the engine and prohibits the engine from being started using any other method (such as using an unregistered key or by shorting the starter relay circuit).
• The system is composed of the transponder equipped key, the coil antenna, and the PCM.
• If there is a malfunction in the system, the security light will display the DTC by flashing when the ignition switch is turned to the ON position. Also, the DTC can be displayed using the SST (WDS).