#
THROTTLE BODY FUNCTION [L8, LF, L3]

id0113z1101500
• A throttle body with a single, electronic-control, motor-operated valve has been adopted in place of the previous cable-controlled throttle valve type.
• Since IAC control during idling is performed by the throttle valve, there is no IAC valve.
• The PCM determines the throttle valve opening angle based on driving conditions, and operates the motor accordingly.
• The throttle valve opening angle is feedback to the PCM by the TP sensor.